{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Power and Cooling","Rotor HP","Cooling Calculations","Manifold Pressure","Performance"],"not_rendered":{"macros":1,"external_links":2,"defined_names":30,"comments":8},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Power and Cooling","index":0,"n_rows":56,"n_cols":23,"rows_kept":56,"merged":[[5,2,5,7],[6,2,6,7],[6,11,7,11],[7,2,7,7],[7,17,10,17],[7,18,10,18],[8,2,8,7],[9,2,9,7],[9,10,10,10],[9,11,10,11],[9,12,10,12],[9,13,10,13],[9,14,10,14],[9,15,10,15],[9,16,10,16],[10,2,10,7],[16,2,21,8],[36,2,37,3]],"flags":["formulas_cached_only"]}
[]
[null,null,"Power and Heat Rejection Requirements Calculator",{"$nulls":14},"Results"]
[null,null," ",null,"Rotary Engine -16B (1600 cc)",{"$nulls":5},"AF =",12.65,"Temp F =",80,null," "]
[{"$nulls":10},"Gear Ratio =",2.85,"Manifold",{"v":29,"d":"29.00"},"\"Hg"," "]
[{"$nulls":10},"Number Rotors =",2]
[null,null,"Air Fuel Mixture Ratio(Air Part)",{"$nulls":5},12.65,12.65]
[null,null,"Initial Engine RPM",{"$nulls":5},5500,5000,null,"Prop Torque",{"$nulls":3}," Engine Torque ",null," "," "," "]
[null,null,"RPM Step",{"$nulls":5},100,100,{"$nulls":5},"(max rpm)",null,"Radiator  Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"," "]
[" ",null,"Manifold Pressure Inches Mercury \" Hg",{"$nulls":5},{"v":29,"d":"29.00"},29.92,null,{"v":575.7563334708617,"d":"576"},{"$nulls":3},{"v":202.01976613012692,"d":"202"},{"$nulls":3},"  "]
[null,null,"Enter Air Temperature(Fahrenheit)",{"$nulls":5},80,59,"Engine RPM","Prop RPM","Air Flow CFM","Air Mass lbm/Min","Fuel Flow Lbm/min","Horse Power ","Gallon/Hour"]
[null,null,"Turbo",{"$nulls":5},"NO","NO",{"$nulls":9}," "]
[null,null,"Message:  ","",{"$nulls":4}," ",null,5500,{"v":1929.8245614035088,"d":"1930"},{"v":295.20645254629625,"d":"295.2"},{"v":21.06401690638104,"d":"21.06"},{"v":1.665139676393758,"d":"1.67"},{"v":179.01159779238202,"d":"179"},{"v":16.65139676393758,"d":"16.7"},{"v":5483.860000923442,"d":"5484"},{"v":2741.930000461721,"d":"2742"}]
[null,null,"Number Rotors",{"$nulls":5},2,2,5600,{"v":1964.9122807017543,"d":"1965"},{"v":300.5738425925926,"d":"300.6"},{"v":21.44699903195161,"d":"21.45"},{"v":1.6954149432372814,"d":"1.70"},{"v":182.26635411587995,"d":"182"},{"v":16.954149432372812,"d":"17.0"},{"v":5583.566546394781,"d":"5584"},{"v":2791.7832731973904,"d":"2792"}]
[null,null,"Gear Ratio ",{"$nulls":5},2.85,2.17,5700,2000,{"v":305.9412326388889,"d":"305.9"},{"v":21.829981157522173,"d":"21.83"},{"v":1.7256902100808043,"d":"1.73"},{"v":185.52111043937782,"d":"186"},{"v":17.25690210080804,"d":"17.3"},{"v":5683.273091866115,"d":"5683"},{"v":2841.6365459330573,"d":"2842"},"  "]
[{"$nulls":10},5800,{"v":2035.0877192982455,"d":"2035"},{"v":311.3086226851852,"d":"311.3"},{"v":22.212963283092737,"d":"22.21"},{"v":1.7559654769243271,"d":"1.76"},{"v":188.77586676287567,"d":"189"},{"v":17.559654769243274,"d":"17.6"},{"v":5782.979637337451,"d":"5783"},{"v":2891.4898186687255,"d":"2891"}]
[null,null,"Version 3.0  Copyright Oct 2007 by Edward L. Anderson",{"$nulls":7},5900,{"v":2070.175438596491,"d":"2070"},{"v":316.6760127314815,"d":"316.7"},{"v":22.5959454086633,"d":"22.60"},{"v":1.7862407437678498,"d":"1.79"},{"v":192.03062308637348,"d":"192"},{"v":17.862407437678495,"d":"17.9"},{"v":5882.686182808785,"d":"5883"},{"v":2941.3430914043925,"d":"2941"}]
[null,null,"FOR EDUCATIONAL AND ENTERTAINMENT PURPOSES ONLY                                                                      This spreadsheet is designed to provide first order estimates of engine power and BTU Heat rejection requirements for a Mazda Wankel 13B Normally aspired engine. It will provide an estimate for Sea Level Power and Power at Altitude MSL. Note: Engine load is not a computational factor, but can be approximated to some degree by manifold pressure.  Enter your desired parameters in the blue Data Input Box.  Copyright @ January, 19, 1994",{"$nulls":7},6000,{"v":2105.2631578947367,"d":"2105"},{"v":322.04340277777777,"d":"322.0"},{"v":22.978927534233865,"d":"22.98"},{"v":1.8165160106113727,"d":"1.82"},{"v":195.28537940987135,"d":"195"},{"v":18.165160106113728,"d":"18.2"},{"v":5982.392728280122,"d":"5982"},{"v":2991.196364140061,"d":"2991"}]
[{"$nulls":9}," ",6100,{"v":2140.3508771929824,"d":"2140"},{"v":327.41079282407406,"d":"327.4"},{"v":23.36190965980443,"d":"23.36"},{"v":1.8467912774548956,"d":"1.85"},{"v":198.54013573336923,"d":"199"},{"v":18.467912774548957,"d":"18.5"},{"v":6082.099273751457,"d":"6082"},{"v":3041.0496368757285,"d":"3041"}]
[{"$nulls":10},6200,{"v":2175.438596491228,"d":"2175"},{"v":332.77818287037036,"d":"332.8"},{"v":23.744891785374996,"d":"23.74"},{"v":1.8770665442984187,"d":"1.88"},{"v":201.7948920568671,"d":"202"},{"v":18.770665442984185,"d":"18.8"},{"v":6181.805819222792,"d":"6182"},{"v":3090.902909611396,"d":"3091"}]
[{"$nulls":10},6300,{"v":2210.5263157894738,"d":"2211"},{"v":338.14557291666665,"d":"338.1"},{"v":24.127873910945556,"d":"24.13"},{"v":1.9073418111419413,"d":"1.91"},{"v":205.0496483803649,"d":"205"},{"v":19.073418111419414,"d":"19.1"},{"v":6281.512364694127,"d":"6282"},{"v":3140.7561823470637,"d":"3141"}]
[{"$nulls":10},6400,{"v":2245.614035087719,"d":"2246"},{"v":343.51296296296294,"d":"343.5"},{"v":24.510856036516124,"d":"24.51"},{"v":1.9376170779854645,"d":"1.94"},{"v":208.3044047038628,"d":"208"},{"v":19.376170779854647,"d":"19.4"},{"v":6381.218910165462,"d":"6381"},{"v":3190.609455082731,"d":"3191"},null,null," "," "]
[{"$nulls":10},6500,{"v":2280.7017543859647,"d":"2281"},{"v":348.8803530092593,"d":"348.9"},{"v":24.893838162086688,"d":"24.89"},{"v":1.9678923448289871,"d":"1.97"},{"v":211.55916102736066,"d":"212"},{"v":19.67892344828987,"d":"19.7"},{"v":6480.925455636799,"d":"6481"},{"v":3240.4627278183993,"d":"3240"}]
[]
[{"$nulls":4}," ",{"$nulls":3}," ",{"$nulls":12},"  "]
[{"$nulls":3},"  ",{"$nulls":5}," "," "]
[{"$nulls":4},"Cooling Capacity Calculator",{"$nulls":13},"Radiator/Cooler Data"]
[{"$nulls":22},"GM evaporator core - Width = 10.5, Height = 9.0 inches"]
[{"$nulls":3},"Note Cooling Capacity is based on two GM evaporator cores and one stock RX-7 Oil cooler",{"$nulls":15},"Enter Surface Area Data",null,null,"two normally used."]
[{"$nulls":3},"(Note: RPM Entered must appear in RESULTS Table - change RPM starting point or step increment to ensure this- if required)",{"$nulls":15},"Fin Area Only",null,null,"Note:  Cooling capacity based soley on Mass flow"]
[{"$nulls":3},"(This rpm should represent the RPM you encounter or expect for the Regime of flight you are in such as Take-0ff, Climb, Cruise, etc)",{"$nulls":15},"Width (nches)",11,null,"through radiator surface area which can be affected by"]
[{"$nulls":3},"(For example your RPM on climbout may be 5600 rpm but your airspeed may only be 120 MPH indicated, where as you may still)",{"$nulls":15},"Height(Inches)",9,null,"a number of factors not taken into consideration in"]
[{"$nulls":3},"(Have an engine rpm of 5600 at cruise, but your airspeed would be more like 170 MPH Indicated.)",{"$nulls":15}," ",null,null,"this simple cooling capacity calculator"]
[{"$nulls":3},"(The selection of this rpm is important for the cooling calculation as it determines the BTU of waste heat rejection required)",{"$nulls":15},"Number of Rads",2,null,"Number of radiators of size entered"]
[{"$nulls":19},"Number of Oil Coolers     ",1,null,"Note: Oil coolers are assumed to be stock RX-7"]
[null,null,"Indicated Air Speed ",null,124,"MPH","",null,null,"Total Cooling Capacity (Radiators and oil Cooler)"]
[null,null,"Altitude MSL",null,0,"Feet"]
[null,null,"Engine RPM of Operating Regime",null,6000,"RPM","HP","Fuel GPH",null,null,"Total Heat Rejection Capacity",null,null,{"v":9046.971087000002,"d":"9047"},"BTU/Minute",{"$nulls":4}," "]
[{"$nulls":6},{"v":195.28537940987135,"d":"195"},{"v":18.165160106113728,"d":"18.17"},{"$nulls":11}," "]
[{"$nulls":10},"Total Heat Rejection Requried",null,null,{"v":8973.589092420183,"d":"8974"},"BTU/Minute"]
[]
[{"$nulls":10},"Overall System Cooling Status",null,null,"Cooling",""]
[]
[{"$nulls":10},"Delta Capacity",null,null,{"v":0.008177552351021175,"d":"0.82%"}]
[]
[]
[null,null,"Radiator Data",{"$nulls":6},"Oil Cooler Data",{"$nulls":9}," "]
[]
[null,null,"Heat Rejection Data",{"$nulls":6},"Heat Rejection Data"]
[]
[{"$nulls":3},"Heat Rejection Capability ",null,null,{"v":6133.539720000001,"d":"6134"},"BTU/Minute "," ",null,"Heat Rejection Capability ",null,null,{"v":2913.431367,"d":"2913"},"BTU/Minute ",null," ",null,null," "]
[{"$nulls":6}," "," ",{"$nulls":5}," "," ",{"$nulls":5}," "," "]
[{"$nulls":3},"Heat Rejection Required ",null,null,{"v":5982.392728280122,"d":"5982"},"BTU/Minute "," ",null,"Heat Rejection Required ",null,null,{"v":2991.196364140061,"d":"2991"},"BTU/Minute",null," ",null,null," "," "," "]
[]
[{"$nulls":3},"Cooling Status",null,null,"Cooling","",null,null,"Cooling Status",null,null,"","Overheating"]
[]
[{"$nulls":3},"Delta Capacity",null,null,{"v":0.025265307475614618,"d":"2.53%"},{"$nulls":3},"Delta Capacity",null,null,{"v":-0.025997957898166172,"d":"-2.60%"}]

{"sheet":"Rotor HP","index":1,"n_rows":153,"n_cols":46,"rows_kept":153,"hidden":true,"merged":[[0,2,0,10],[1,2,1,10],[1,15,1,17],[2,3,2,9],[3,2,3,9],[5,3,5,8],[5,13,6,13],[5,17,6,17],[5,18,6,18],[6,3,6,8],[7,3,7,8],[8,3,8,8],[9,3,9,8],[10,3,10,8],[11,3,11,8],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[74,17,74,18],[77,0,78,0],[89,6,89,8],[89,13,89,15],[90,6,90,8],[90,13,90,15],[91,6,91,8],[91,13,91,15],[92,6,92,8],[92,13,92,15],[93,6,93,8],[93,13,93,15],[94,6,94,8],[94,13,94,15],[95,13,95,15],[96,13,96,15],[97,13,97,15],[98,13,98,15],[99,13,99,15],[100,13,100,15],[101,13,101,15],[102,13,102,15],[103,13,103,15],[104,13,104,15],[105,13,105,15],[106,13,106,15],[107,13,107,15],[108,13,108,15],[109,13,109,15],[110,13,110,15],[111,13,111,15],[112,13,112,15],[113,13,113,15],[115,17,118,18],[127,8,127,9],[128,8,128,9]],"flags":["formulas_cached_only"]}
[null,null,"Mazda Wankel Rotary Engine Performance Spreadsheet Version 1.5 Mar 2001"]
[null,null,"  FOR EDUCATIONAL AND ENTERTAINMENT PURPOSES ONLY                                                                      This spreadsheet is designed to provide first order estimates of engine power and BTU Heat rejection requirements for a Mazda Wankel 13B Normally aspired engine. It will provide an estimate for Sea Level Power and Power at Altitude MSL. Note: Engine load is not a computational factor, but can be approximated to some degree by varying the throttle setting.  Enter your desired parameters in the blue Data Input Box.  Copywrite @ January, 19, 1994",{"$nulls":12},"Calculation Results"]
[null," ",{"$nulls":11},"AF =",12.65," ","Temp F =",80]
[null,null,"Developed by: Ed Anderson, eanderson@carolina.rr.com, Matthews NC",{"$nulls":10},"Altitude =",0," ","Manifold",{"v":29,"d":"29.00"}]
[{"$nulls":3},"This Spreadsheet is Protected to Preclude Inadvertent erasing of Formulas",{"$nulls":9},"Gear Ratio =",2.85,null,"RESULTS"]
[null,"Default Values",null,"DATA ENTRY BOX",{"$nulls":5}," Enter Data",{"$nulls":3},"Engine RPM",{"$nulls":3},"Radiator Cooler Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"]
[null,13.5,null,"Air Fuel Mixture Ratio(Air Part)",{"$nulls":5},12.65,{"$nulls":4},"Prop RPM","Horse Power/Sec","Gallon/Hour"]
[null,4000,null,"Initial Engine RPM",{"$nulls":5},5500]
[null,250,null,"RPM Step",{"$nulls":5},100,{"$nulls":3},5500,{"v":1929.8245614035088,"d":"1930"},{"v":179.01159779238202,"d":"179"},{"v":16.65139676393758,"d":"16.65"},{"v":5483.860000923442,"d":"5484"},{"v":2741.930000461721,"d":"2742"}," "]
[null,100,null,"% Throttle Opening (Enter Percentage)",{"$nulls":5},{"v":29,"d":"2900%"},{"$nulls":3},5600,{"v":1964.9122807017543,"d":"1965"},{"v":182.26635411587995,"d":"182"},{"v":16.954149432372812,"d":"16.95"},{"v":5583.566546394781,"d":"5584"},{"v":2791.7832731973904,"d":"2792"}]
[null,0,null,"MSL Altitude in feet",{"$nulls":5},0,{"$nulls":3},5700,2000,{"v":185.52111043937782,"d":"186"},{"v":17.25690210080804,"d":"17.26"},{"v":5683.273091866115,"d":"5683"},{"v":2841.6365459330573,"d":"2842"}]
[null,60,null,"Enter Air Temperature (Select 15F - 100F, in 5 Degree  Increments)",{"$nulls":5},80,{"$nulls":3},5800,{"v":2035.0877192982455,"d":"2035"},{"v":188.77586676287567,"d":"189"},{"v":17.559654769243274,"d":"17.56"},{"v":5782.979637337451,"d":"5783"},{"v":2891.4898186687255,"d":"2891"}]
[null,{"v":0,"d":"0.000"},null,"Enter Boost (psi Gauge)  Calculations Compensate for Altitude",{"$nulls":5},0,1.042982456140351,null,null,5900,{"v":2070.175438596491,"d":"2070"},{"v":192.03062308637348,"d":"192"},{"v":17.862407437678495,"d":"17.86"},{"v":5882.686182808785,"d":"5883"},{"v":2941.3430914043925,"d":"2941"}]
[{"$nulls":13},6000,{"v":2105.2631578947367,"d":"2105"},{"v":195.28537940987135,"d":"195"},{"v":18.165160106113728,"d":"18.17"},{"v":5982.392728280122,"d":"5982"},{"v":2991.196364140061,"d":"2991"}]
[{"$nulls":3},"Step 1 Enter Air/Fuel Ratio (Air Value)",{"$nulls":9},6100,{"v":2140.3508771929824,"d":"2140"},{"v":198.54013573336923,"d":"199"},{"v":18.467912774548957,"d":"18.47"},{"v":6082.099273751457,"d":"6082"},{"v":3041.0496368757285,"d":"3041"}]
[{"$nulls":3},"Step 2 Enter RPM Start Value",{"$nulls":9},6200,{"v":2175.438596491228,"d":"2175"},{"v":201.7948920568671,"d":"202"},{"v":18.770665442984185,"d":"18.77"},{"v":6181.805819222792,"d":"6182"},{"v":3090.902909611396,"d":"3091"}]
[{"$nulls":3},"Step 3 Enter RPM Step Increment",{"$nulls":9},6300,{"v":2210.5263157894738,"d":"2211"},{"v":205.0496483803649,"d":"205"},{"v":19.073418111419414,"d":"19.07"},{"v":6281.512364694127,"d":"6282"},{"v":3140.7561823470637,"d":"3141"}," "]
[{"$nulls":3},"Step 4 Enter Throttle Opening %",{"$nulls":9},6400,{"v":2245.614035087719,"d":"2246"},{"v":208.3044047038628,"d":"208"},{"v":19.376170779854647,"d":"19.38"},{"v":6381.218910165462,"d":"6381"},{"v":3190.609455082731,"d":"3191"}]
[{"$nulls":3},"Step 5 Enter MSL Operating Altitude in thousand of feet",{"$nulls":9},6500,{"v":2280.7017543859647,"d":"2281"},{"v":211.55916102736066,"d":"212"},{"v":19.67892344828987,"d":"19.68"},{"v":6480.925455636799,"d":"6481"},{"v":3240.4627278183993,"d":"3240"}]
[{"$nulls":3},"Step 6 Enter OAT F between 15 -100 in 5 degree increments",{"$nulls":9},6600,{"v":2315.7894736842104,"d":"2316"},{"v":214.8139173508585,"d":"215"},{"v":19.9816761167251,"d":"19.98"},{"v":6580.632001108133,"d":"6581"},{"v":3290.3160005540667,"d":"3290"}]
[{"$nulls":3},"Step 7 Enter Gauge Boost in PSI (Note: No intercooler in calculation)",{"$nulls":9},6700,{"v":2350.877192982456,"d":"2351"},{"v":218.06867367435632,"d":"218"},{"v":20.28442878516033,"d":"20.28"},{"v":6680.338546579467,"d":"6680"},{"v":3340.1692732897336,"d":"3340"}]
[{"$nulls":13},6800,{"v":2385.964912280702,"d":"2386"},{"v":221.3234299978542,"d":"221"},{"v":20.587181453595555,"d":"20.59"},{"v":6780.045092050804,"d":"6780"},{"v":3390.022546025402,"d":"3390"}]
[{"$nulls":3},"NOTES  Below"]
[{"$nulls":3},"Number of Rotors",{"$nulls":4}," ",null," "]
[{"$nulls":3},"Fuel Injection Parameters Note"]
[{"$nulls":3},"Power Assumptions"]
[{"$nulls":3},"Assumed Max Power",{"$nulls":12},"Manifold Pressure/Power Estimates"]
[{"$nulls":15}," ",null,0]
[{"$nulls":13}," Assumed Max Engine Power",null,180,"Temp F",80,"Specified Max RPM for Look Up Table",6400]
[{"$nulls":13},"A/F Ratio",null,12.65,"Altitude","Sea Level","Throttle",{"v":29,"d":"2900%"}]
[{"$nulls":15},"% Engine Power","HP","Inches HG","RPM"]
[{"$nulls":15},{"v":1.1572466927992378,"d":"116%"},{"v":208.3044047038628,"d":"208"},29,6400," "]
[{"$nulls":15},{"v":1.1173416344268503,"d":"112%"},{"v":201.12149419683305,"d":"201"},28,{"v":6179.310344827586,"d":"6179"}]
[{"$nulls":15},{"v":1.0774365760544626,"d":"108%"},{"v":193.93858368980327,"d":"194"},27,{"v":5958.620689655171,"d":"5959"}]
[{"$nulls":15},{"v":1.0375315176820752,"d":"104%"},{"v":186.75567318277353,"d":"187"},26,{"v":5737.931034482759,"d":"5738"}]
[{"$nulls":15},{"v":0.9976264593096876,"d":"100%"},{"v":179.57276267574377,"d":"180"},25,{"v":5517.241379310344,"d":"5517"}]
[{"$nulls":15},{"v":0.9577214009373001,"d":"96%"},{"v":172.38985216871401,"d":"172"},24,{"v":5296.55172413793,"d":"5297"}]
[{"$nulls":15},{"v":0.9178163425649127,"d":"92%"},{"v":165.20694166168428,"d":"165"},23,{"v":5075.862068965517,"d":"5076"}]
[{"$nulls":15},{"v":0.8779112841925252,"d":"88%"},{"v":158.02403115465452,"d":"158"},22,{"v":4855.172413793103,"d":"4855"}]
[{"$nulls":15},{"v":0.8380062258201377,"d":"84%"},{"v":150.8411206476248,"d":"151"},21,{"v":4634.482758620689,"d":"4634"}]
[{"$nulls":15},{"v":0.7981011674477502,"d":"80%"},{"v":143.65821014059503,"d":"144"},20,{"v":4413.793103448276,"d":"4414"}]
[{"$nulls":15},{"v":0.7581961090753626,"d":"76%"},{"v":136.47529963356527,"d":"136"},19,{"v":4193.103448275862,"d":"4193"}]
[{"$nulls":15},{"v":0.7182910507029752,"d":"72%"},{"v":129.29238912653554,"d":"129"},18,{"v":3972.4137931034484,"d":"3972"}]
[{"$nulls":15},{"v":0.6783859923305876,"d":"68%"},{"v":122.10947861950577,"d":"122"},17,{"v":3751.724137931034,"d":"3752"}]
[{"$nulls":15},{"v":0.6384809339582002,"d":"64%"},{"v":114.92656811247602,"d":"115"},16,{"v":3531.0344827586205,"d":"3531"}]
[{"$nulls":15},{"v":0.5985758755858126,"d":"60%"},{"v":107.74365760544627,"d":"108"},15,{"v":3310.3448275862065,"d":"3310"}]
[{"$nulls":15},{"v":0.5586708172134252,"d":"56%"},{"v":100.56074709841653,"d":"101"},14,{"v":3089.655172413793,"d":"3090"}]
[{"$nulls":15},{"v":0.5187657588410376,"d":"52%"},{"v":93.37783659138677,"d":"93"},13,{"v":2868.9655172413795,"d":"2869"}]
[{"$nulls":15},{"v":0.47886070046865004,"d":"48%"},{"v":86.19492608435701,"d":"86"},12,{"v":2648.275862068965,"d":"2648"}]
[{"$nulls":15},{"v":0.4389556420962626,"d":"44%"},{"v":79.01201557732726,"d":"79"},11,{"v":2427.5862068965516,"d":"2428"}]
[{"$nulls":15},{"v":0.3990505837238751,"d":"40%"},{"v":71.82910507029752,"d":"72"},10,{"v":2206.896551724138,"d":"2207"}]
[{"$nulls":15},{"v":0.3591455253514876,"d":"36%"},{"v":64.64619456326777,"d":"65"},9,{"v":1986.2068965517242,"d":"1986"}]
[{"$nulls":15},{"v":0.3192404669791001,"d":"32%"},{"v":57.46328405623801,"d":"57"},8,{"v":1765.5172413793102,"d":"1766"}]
[{"$nulls":15},{"v":0.2793354086067126,"d":"28%"},{"v":50.280373549208264,"d":"50"},7,{"v":1544.8275862068965,"d":"1545"}]
[{"$nulls":15},{"v":0.23943035023432502,"d":"24%"},{"v":43.097463042178504,"d":"43"},6,{"v":1324.1379310344826,"d":"1324"}]
[{"$nulls":15},{"v":0.19952529186193754,"d":"20%"},{"v":35.91455253514876,"d":"36"},5,{"v":1103.448275862069,"d":"1103"}]
[{"$nulls":15},{"v":0.15962023348955004,"d":"16%"},{"v":28.731642028119005,"d":"29"},4,{"v":882.7586206896551,"d":"883"}]
[{"$nulls":15},{"v":0.11971517511716251,"d":"12%"},{"v":21.548731521089252,"d":"22"},3,{"v":662.0689655172413,"d":"662"}]
[{"$nulls":15},{"v":0.07981011674477502,"d":"8%"},{"v":14.365821014059502,"d":"14"},2,{"v":441.37931034482756,"d":"441"}]
[{"$nulls":15},{"v":0.03990505837238751,"d":"4%"},{"v":7.182910507029751,"d":"7"},1,{"v":220.68965517241378,"d":"221"}]
[]
[]
[]
[]
[]
[]
[{"$nulls":13},"Calculation Parameters and Equations"]
[]
[]
[{"$nulls":22}," "," "]
[null,"Turbo Charger Density Compensation",{"$nulls":16}," ",{"$nulls":3}," "]
["P1 At Altitude",{"v":14.738916256157637,"d":"14.74"},29.9992091417848,29.92," "," ",{"$nulls":3},"Spreadsheet for calculating Engine Power, BTU cooling, and injector Timing",{"$nulls":12}," "]
["P2 psi Gauge",0,0,1,0,{"$nulls":4},"Parameter","Units","Value","Air Density                                                    Factor","Conversion Values",{"$nulls":3},"Engines 16B (2 Rotors) , 20G (3 Rotors)",{"$nulls":4}," "]
[2.035374149659864,{"$nulls":6},"=L74*(-3*10^(-5)*$J$11+1)",null,"Air Mass Pa (Sea Level)","Lbm/Ft^3",{"v":0.07341600000000001,"d":"0.073416"},0.00228,"Gasoline Energy",null,null,"19000 Btu/lbm-sec","VC=Rotor Chamber volume CID",null,48.815," "]
[null,null,"Delta T Ideal",null,"Delta T Real",{"$nulls":3},"Compensate for altitude ","Air Mass Pa  (Altitude MSL) ","Lbm/Ft^3",{"v":0.07341600000000001,"d":"0.073416"},0.9587888982338099,"1 Btu =",null,null,"778 ft-lb","R = Number of Rotors",null,{"v":2,"d":"2.000"}," ",{"$nulls":3}," "]
["T1 Inlet Temp F",80,0,null,0,null,null,{"v":0.07341600000000001,"d":"0.073416"},null,"Fuel Mass Pf","Lbm/Ft^3",44.883,null,"1 Horse Power =",null,null,"550 ft-lb ","F = Faces Per Rotor",null,{"v":3,"d":"3.000"}]
[{"$nulls":9},"Temperature","Degrees F",null,{"v":80,"d":"80.000"},{"$nulls":4},"Total Swept Chamber Volume per Rotor Rev - Single Rotor",null,146.445,"Read Note -->"]
["Compressor Efficiency",65,{"$nulls":7},"Fuel/Air Ratio",null,{"v":0.07905138339920949,"d":"0.079"},{"$nulls":5},"VCID=Total Displacement for N rotors per Rotor rev",null,{"v":292.89,"d":"292.890"},{"$nulls":4}," "]
[{"$nulls":8}," ","  Fuel",null,{"v":1,"d":"1.000"},{"$nulls":5},"AirDisplacement per Rotor Revolution (Cubic Feet)",null,{"v":0.16949652777777777,"d":"0.169"},{"$nulls":3}," "]
[{"$nulls":9},"  Air",null,null,{"v":12.65,"d":"12.650"}]
["T2 Oulet Temp F",80,{"$nulls":6}," "]
[{"$nulls":9},"Engine RPM/Airflow Calculations",{"$nulls":9}," "]
[{"$nulls":21}," "]
[null,null,"Temp Ratio","Pressure Ratio",{"$nulls":5},"Operating parameters",null," ",{"$nulls":7}," "]
["Density Ratio",1,1,1,{"$nulls":5},"Intake 'Efficiency Ve",null,null,{"v":0.95,"d":"95.00%"},"was 100%"]
[{"$nulls":9},"Vt Throttle % Open",null,{"v":0.9719068208617896,"d":"0.972"},{"v":0.9719068208617896,"d":"97.19%"},"was Thottle % open"]
["Sea level air Density",{"v":0.07341600000000001,"d":"0.073416"},{"$nulls":7},"RPM Start Value",null,null,{"v":5500,"d":"5500.000"}]
[{"$nulls":9},"RPM Step Value",null,null,{"v":100,"d":"100.000"}," "]
["Altitude Density",{"v":0.07341600000000001,"d":"0.073"}]
["Turbo Density",0.07341600000000001,{"$nulls":4},"Once parameters are set for",null,null,"Engine RPM (Calculation",{"$nulls":3},"Eng RPM",null,null,5500,5600,5700,5800,5900,6000,6100,6200,6300,6400,6500,6600,6700,6800,null,"RPM",5500,5600,5700,5800,5900,6000,6100,6200,6300,6400,6500,6600,6700,6800]
[{"$nulls":6},"an engine configuration then",null,null,"Propeller RPM (PSRU Ratio = 2.17)",{"v":2.17,"d":"2.170"},null,null,"Prop RPM",null,null,{"v":2534.562211981567,"d":"2535"},{"v":2580.6451612903224,"d":"2581"},{"v":2626.7281105990783,"d":"2627"},{"v":2672.811059907834,"d":"2673"},{"v":2718.89400921659,"d":"2719"},{"v":2764.9769585253457,"d":"2765"},{"v":2811.0599078341015,"d":"2811"},{"v":2857.1428571428573,"d":"2857"},{"v":2903.225806451613,"d":"2903"},{"v":2949.308755760369,"d":"2949"},{"v":2995.3917050691243,"d":"2995"},{"v":3041.47465437788,"d":"3041"},{"v":3087.557603686636,"d":"3088"},{"v":3133.6405529953918,"d":"3134"},null,"AirFlow CFM",{"v":295.20645254629625,"d":"295"},{"v":300.5738425925926,"d":"301"},{"v":305.9412326388889,"d":"306"},{"v":311.3086226851852,"d":"311"},{"v":316.6760127314815,"d":"317"},{"v":322.04340277777777,"d":"322"},{"v":327.41079282407406,"d":"327"},{"v":332.77818287037036,"d":"333"},{"v":338.14557291666665,"d":"338"},{"v":343.51296296296294,"d":"344"},{"v":348.8803530092593,"d":"349"},{"v":354.24774305555553,"d":"354"},{"v":359.6151331018518,"d":"360"},{"v":364.9825231481481,"d":"365"}]
[{"$nulls":6},"Normally only need to vary RPM",null,null,"Air Flow CFM",null,null," ","Air Flow CFM",null,null,{"v":295.20645254629625,"d":"295"},{"v":300.5738425925926,"d":"301"},{"v":305.9412326388889,"d":"306"},{"v":311.3086226851852,"d":"311"},{"v":316.6760127314815,"d":"317"},{"v":322.04340277777777,"d":"322"},{"v":327.41079282407406,"d":"327"},{"v":332.77818287037036,"d":"333"},{"v":338.14557291666665,"d":"338"},{"v":343.51296296296294,"d":"344"},{"v":348.8803530092593,"d":"349"},{"v":354.24774305555553,"d":"354"},{"v":359.6151331018518,"d":"360"},{"v":364.9825231481481,"d":"365"},null,"Runner Dia (inches)",{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"}]
[{"$nulls":6},"Throttle Opening and  ",null,null,"Air Flow Lbm/min",null," "," ","Air Flow Mass",null,null,{"v":21.06401690638104,"d":"21.06"},{"v":21.44699903195161,"d":"21.45"},{"v":21.829981157522173,"d":"21.83"},{"v":22.212963283092737,"d":"22.21"},{"v":22.5959454086633,"d":"22.60"},{"v":22.978927534233865,"d":"22.98"},{"v":23.36190965980443,"d":"23.36"},{"v":23.744891785374996,"d":"23.74"},{"v":24.127873910945556,"d":"24.13"},{"v":24.510856036516124,"d":"24.51"},{"v":24.893838162086688,"d":"24.89"},{"v":25.27682028765725,"d":"25.28"},{"v":25.659802413227816,"d":"25.66"},{"v":26.04278453879838,"d":"26.04"},null,"Number Runners",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"}]
[{"$nulls":6},"Perhaps fuel ratio",null,null,"Fuel Required LBM/Min",{"$nulls":3},"Fuel Flow Mass",null,null,{"v":1.665139676393758,"d":"1.67"},{"v":1.6954149432372814,"d":"1.70"},{"v":1.7256902100808043,"d":"1.73"},{"v":1.7559654769243271,"d":"1.76"},{"v":1.7862407437678498,"d":"1.79"},{"v":1.8165160106113727,"d":"1.82"},{"v":1.8467912774548956,"d":"1.85"},{"v":1.8770665442984187,"d":"1.88"},{"v":1.9073418111419413,"d":"1.91"},{"v":1.9376170779854645,"d":"1.94"},{"v":1.9678923448289871,"d":"1.97"},{"v":1.99816761167251,"d":"2.00"},{"v":2.028442878516033,"d":"2.03"},{"v":2.0587181453595558,"d":"2.06"},null,"Runner Air Velocity(Feet/Sec)",{"v":288.66703045856923,"d":"288.667"},{"v":293.91552192145235,"d":"293.916"},{"v":299.1640133843354,"d":"299.164"},{"v":304.4125048472185,"d":"304.413"},{"v":309.66099631010155,"d":"309.661"},{"v":314.9094877729846,"d":"314.909"},{"v":320.1579792358677,"d":"320.158"},{"v":325.40647069875075,"d":"325.406"},{"v":330.6549621616339,"d":"330.655"},{"v":335.90345362451694,"d":"335.903"},{"v":341.15194508740007,"d":"341.152"},{"v":346.4004365502831,"d":"346.400"},{"v":351.64892801316614,"d":"351.649"},{"v":356.8974194760492,"d":"356.897"}]
[{"$nulls":6},"from Data Input-Results Spreadsheet",null,null,"  Gallon/Min",{"$nulls":3},"Gallon/Min",null,null,{"v":0.27752327939895965,"d":"0.28"},{"v":0.28256915720621356,"d":"0.28"},{"v":0.28761503501346736,"d":"0.29"},{"v":0.2926609128207212,"d":"0.29"},{"v":0.29770679062797495,"d":"0.30"},{"v":0.3027526684352288,"d":"0.30"},{"v":0.3077985462424826,"d":"0.31"},{"v":0.31284442404973645,"d":"0.31"},{"v":0.31789030185699024,"d":"0.32"},{"v":0.3229361796642441,"d":"0.32"},{"v":0.32798205747149783,"d":"0.33"},{"v":0.3330279352787517,"d":"0.33"},{"v":0.3380738130860055,"d":"0.34"},{"v":0.3431196908932593,"d":"0.34"},null,"Runner Air Velocity MPH",{"v":196.81842985811537,"d":"196.818"},{"v":200.39694676462662,"d":"200.397"},{"v":203.9754636711378,"d":"203.975"},{"v":207.55398057764896,"d":"207.554"},{"v":211.13249748416015,"d":"211.132"},{"v":214.71101439067132,"d":"214.711"},{"v":218.28953129718252,"d":"218.290"},{"v":221.8680482036937,"d":"221.868"},{"v":225.44656511020492,"d":"225.447"},{"v":229.0250820167161,"d":"229.025"},{"v":232.6035989232273,"d":"232.604"},{"v":236.18211582973848,"d":"236.182"},{"v":239.76063273624962,"d":"239.761"}]
[{"$nulls":8},"  ","  Gallon/Hour",{"$nulls":3},"Gallon/Hour",null,null,{"v":16.65139676393758,"d":"16.65"},{"v":16.954149432372812,"d":"16.95"},{"v":17.25690210080804,"d":"17.26"},{"v":17.559654769243274,"d":"17.56"},{"v":17.862407437678495,"d":"17.86"},{"v":18.165160106113728,"d":"18.17"},{"v":18.467912774548957,"d":"18.47"},{"v":18.770665442984185,"d":"18.77"},{"v":19.073418111419414,"d":"19.07"},{"v":19.376170779854647,"d":"19.38"},{"v":19.67892344828987,"d":"19.68"},{"v":19.9816761167251,"d":"19.98"},{"v":20.28442878516033,"d":"20.28"},{"v":20.587181453595555,"d":"20.59"},null,"Runner Air Velocity (inches/sec)",{"v":3464.0043655028308,"d":"3464.004"},{"v":3526.986263057428,"d":"3526.986"},{"v":3589.968160612025,"d":"3589.968"},{"v":3652.9500581666216,"d":"3652.950"},{"v":3715.9319557212184,"d":"3715.932"},{"v":3778.913853275815,"d":"3778.914"},{"v":3841.895750830412,"d":"3841.896"},{"v":3904.877648385009,"d":"3904.878"},{"v":3967.8595459396065,"d":"3967.860"},{"v":4030.8414434942033,"d":"4030.841"},{"v":4093.823341048801,"d":"4093.823"},{"v":4156.805238603397,"d":"4156.805"},{"v":4219.787136157994,"d":"4219.787"},{"v":4282.7690337125905,"d":"4282.769"}]
[]
[{"$nulls":9},"Power/Heat Calculations",{"$nulls":31},{"v":171.75648148148147,"d":"171.756"},"cfpm"]
[{"$nulls":9},"BTU/sec ",{"$nulls":3},"BTU/Second",null,null,{"v":527.2942308580234,"d":"527"},{"v":536.8813986918058,"d":"537"},{"v":546.468566525588,"d":"546"},{"v":556.0557343593703,"d":"556"},{"v":565.6429021931524,"d":"566"},{"v":575.2300700269348,"d":"575"},{"v":584.817237860717,"d":"585"},{"v":594.4044056944992,"d":"594"},{"v":603.9915735282814,"d":"604"},{"v":613.5787413620637,"d":"614"},{"v":623.165909195846,"d":"623"},{"v":632.7530770296282,"d":"633"},{"v":642.3402448634104,"d":"642"},{"v":651.9274126971926,"d":"652"},{"$nulls":9},1.25,1.227184630308513,{"v":2.8626080246913577,"d":"2.863"},"cfps"]
[{"$nulls":9},"Torque Ft-lbs",{"$nulls":3},"Torque (Ft-Lbs)",null,null,{"v":410234.9116075422,"d":"410235"},{"v":417693.7281822249,"d":"417694"},{"v":425152.5447569075,"d":"425153"},{"v":432611.36133159004,"d":"432611"},{"v":440070.1779062726,"d":"440070"},{"v":447528.99448095524,"d":"447529"},{"v":454987.81105563784,"d":"454988"},{"v":462446.62763032044,"d":"462447"},{"v":469905.4442050029,"d":"469905"},{"v":477364.2607796856,"d":"477364"},{"v":484823.0773543682,"d":"484823"},{"v":492281.89392905077,"d":"492282"},{"v":499740.71050373325,"d":"499741"},{"v":507199.52707841585,"d":"507200"},{"$nulls":9},1.5,1.7671458676442586]
[{"$nulls":9},"Horse Power (Total)",{"$nulls":3},"Horse Power (Total)",null,null,{"v":745.8816574682585,"d":"746"},{"v":759.4431421494999,"d":"759"},{"v":773.0046268307409,"d":"773"},{"v":786.566111511982,"d":"787"},{"v":800.1275961932229,"d":"800"},{"v":813.689080874464,"d":"814"},{"v":827.2505655557052,"d":"827"},{"v":840.8120502369462,"d":"841"},{"v":854.3735349181871,"d":"854"},{"v":867.9350195994283,"d":"868"},{"v":881.4965042806695,"d":"881"},{"v":895.0579889619105,"d":"895"},{"v":908.6194736431513,"d":"909"},{"v":922.1809583243925,"d":"922"},{"$nulls":9},"Area",2.9943304979527716]
[{"$nulls":8},"26","  Useful",{"v":0.24,"d":"24%"},{"v":24,"d":"24.000"},null,"Horse Power (Useful)",null,null,{"v":179.01159779238202,"d":"179"},{"v":182.26635411587995,"d":"182"},{"v":185.52111043937782,"d":"186"},{"v":188.77586676287567,"d":"189"},{"v":192.03062308637348,"d":"192"},{"v":195.28537940987135,"d":"195"},{"v":198.54013573336923,"d":"199"},{"v":201.7948920568671,"d":"202"},{"v":205.0496483803649,"d":"205"},{"v":208.3044047038628,"d":"208"},{"v":211.55916102736066,"d":"212"},{"v":214.8139173508585,"d":"215"},{"v":218.06867367435632,"d":"218"},{"v":221.3234299978542,"d":"221"},{"$nulls":9},"Area ft^2",0.020793961791338692,{"v":137.6653498461135,"d":"137.665"},"fps"]
[{"$nulls":9},"  Cooling Loss",{"v":0.26,"d":"26%"},{"v":26,"d":"26.000"},null,"HP Loss (Cooling)",null,null,{"v":193.92923094174722,"d":"194"},{"v":197.45521695886998,"d":"197"},{"v":200.98120297599263,"d":"201"},{"v":204.5071889931153,"d":"205"},{"v":208.03317501023795,"d":"208"},{"v":211.55916102736066,"d":"212"},{"v":215.08514704448336,"d":"215"},{"v":218.611133061606,"d":"219"},{"v":222.13711907872866,"d":"222"},{"v":225.66310509585136,"d":"226"},{"v":229.18909111297407,"d":"229"},{"v":232.71507713009674,"d":"233"},{"v":236.24106314721934,"d":"236"},{"v":239.76704916434204,"d":"240"}]
[{"$nulls":8},"40","  Exhaust Loss",{"v":0.5,"d":"50%"},{"v":50,"d":"50.000"},null,"HP Loss (Exhaust)",null,null,{"v":372.94082873412924,"d":"373"},{"v":379.72157107474993,"d":"380"},{"v":386.50231341537045,"d":"387"},{"v":393.283055755991,"d":"393"},{"v":400.06379809661144,"d":"400"},{"v":406.844540437232,"d":"407"},{"v":413.6252827778526,"d":"414"},{"v":420.4060251184731,"d":"420"},{"v":427.1867674590936,"d":"427"},{"v":433.96750979971415,"d":"434"},{"v":440.7482521403347,"d":"441"},{"v":447.52899448095525,"d":"448"},{"v":454.30973682157565,"d":"454"},{"v":461.09047916219623,"d":"461"}]
[]
[{"$nulls":4}," ",{"$nulls":4},"Cooling Requirements BTU/Min"]
[{"$nulls":9},"  Total Cooling Rejection BTU",{"$nulls":3},"Total BTU Rejection  BTU/Sec",null,null,{"v":8225.790001385163,"d":"8226"},{"v":8375.349819592171,"d":"8375"},{"v":8524.909637799172,"d":"8525"},{"v":8674.469456006176,"d":"8674"},{"v":8824.029274213177,"d":"8824"},{"v":8973.589092420183,"d":"8974"},{"v":9123.148910627186,"d":"9123"},{"v":9272.708728834188,"d":"9273"},{"v":9422.26854704119,"d":"9422"},{"v":9571.828365248193,"d":"9572"},{"v":9721.388183455198,"d":"9721"},{"v":9870.9480016622,"d":"9871"},{"v":10020.5078198692,"d":"10021"},{"v":10170.067638076205,"d":"10170"}]
[{"$nulls":9},"  Radiator = 2/3 of  Rejection"," ",null,null,"BTU Rejection Radiators",null,null,{"v":5483.860000923442,"d":"5484"},{"v":5583.566546394781,"d":"5584"},{"v":5683.273091866115,"d":"5683"},{"v":5782.979637337451,"d":"5783"},{"v":5882.686182808785,"d":"5883"},{"v":5982.392728280122,"d":"5982"},{"v":6082.099273751457,"d":"6082"},{"v":6181.805819222792,"d":"6182"},{"v":6281.512364694127,"d":"6282"},{"v":6381.218910165462,"d":"6381"},{"v":6480.925455636799,"d":"6481"},{"v":6580.632001108133,"d":"6581"},{"v":6680.338546579467,"d":"6680"},{"v":6780.045092050804,"d":"6780"}]
[{"$nulls":9},"  Oil Cooler = 1/3 of Rejection",{"$nulls":3},"BTU Rejection Oil Cooler",null,null,{"v":2741.930000461721,"d":"2742"},{"v":2791.7832731973904,"d":"2792"},{"v":2841.6365459330573,"d":"2842"},{"v":2891.4898186687255,"d":"2891"},{"v":2941.3430914043925,"d":"2941"},{"v":2991.196364140061,"d":"2991"},{"v":3041.0496368757285,"d":"3041"},{"v":3090.902909611396,"d":"3091"},{"v":3140.7561823470637,"d":"3141"},{"v":3190.609455082731,"d":"3191"},{"v":3240.4627278183993,"d":"3240"},{"v":3290.3160005540667,"d":"3290"},{"v":3340.1692732897336,"d":"3340"},{"v":3390.022546025402,"d":"3390"}]
[]
[{"$nulls":9},"Injector timing "]
[{"$nulls":9},"  Total Fuel Flow Requirement Lbm/Min",{"$nulls":3},"Total Fuel flow Required (Lbm/min)",null,null,{"v":1.665139676393758,"d":"1.67E+00"},{"v":1.6954149432372814,"d":"1.70E+00"},{"v":1.7256902100808043,"d":"1.73E+00"},{"v":1.7559654769243271,"d":"1.76E+00"},{"v":1.7862407437678498,"d":"1.79E+00"},{"v":1.8165160106113727,"d":"1.82E+00"},{"v":1.8467912774548956,"d":"1.85E+00"},{"v":1.8770665442984187,"d":"1.88E+00"},{"v":1.9073418111419413,"d":"1.91E+00"},{"v":1.9376170779854645,"d":"1.94E+00"},{"v":1.9678923448289871,"d":"1.97E+00"},{"v":1.99816761167251,"d":"2.00E+00"},{"v":2.028442878516033,"d":"2.03E+00"},{"v":2.0587181453595558,"d":"2.06E+00"}," "]
[{"$nulls":9},"  Fuel Required lbm/msec",{"$nulls":3},"Fuel Flow Required (Lbm/Millisecond)",null,null,2.7752327939895967e-05,2.8256915720621355e-05,2.876150350134674e-05,2.926609128207212e-05,2.9770679062797497e-05,3.0275266843522878e-05,3.077985462424826e-05,3.1284442404973645e-05,3.178903018569902e-05,3.229361796642441e-05,3.2798205747149786e-05,3.3302793527875164e-05,3.380738130860054e-05,3.431196908932593e-05," "]
[{"$nulls":9},"  On time Required per injector/msec",{"$nulls":3},"On-time per Injector (Millisecond)",null,null,{"v":5.550465587979193,"d":"5.55"},{"v":5.651383144124271,"d":"5.65"},{"v":5.752300700269347,"d":"5.75"},{"v":5.853218256414423,"d":"5.85"},{"v":5.954135812559499,"d":"5.95"},{"v":6.055053368704575,"d":"6.06"},{"v":6.155970924849651,"d":"6.16"},{"v":6.2568884809947285,"d":"6.26"},{"v":6.357806037139804,"d":"6.36"},{"v":6.458723593284881,"d":"6.46"},{"v":6.5596411494299565,"d":"6.56"},{"v":6.660558705575032,"d":"6.66"},{"v":6.761476261720108,"d":"6.76"},{"v":6.862393817865185,"d":"6.86"}," "]
[]
[{"$nulls":9},"Injection Set Up Parameters",{"$nulls":5}," "," ","Fuel Flow Required (Lbm/Millisecond) / Flow Rate (Lbm/Msec) per Injector * Factor for Number of Staged Injectors (Longer times for few injectors) * Inverse of Trigger Divide By"]
[{"$nulls":8},"These value","  Injectors Staged at (RPM) - User Value",null,{"v":3000,"d":"3000.000"},{"$nulls":3}," ","Injector On time ="]
[{"$nulls":8},"only need to","  Ignition Divide by (Haltech) otherwise 1",null,{"v":2,"d":"2.000"},{"$nulls":3}," "," "]
[{"$nulls":8},"be entered","  Injector Flow Rate per Injector Lbs/hr",null,{"v":45,"d":"45.000"}]
[{"$nulls":8},"once per","  80% max Flow Rate Lbs/hr",null,{"v":40.5,"d":"40.500"}]
[{"$nulls":8},"engine ","  Fuel Pressure actuall/45psi",null,40,{"v":0.8888888888888888,"d":"0.889"}]
[{"$nulls":8},"configuration","  Number of injectors",null,{"v":4,"d":"4.000"}]
[{"$nulls":9},"  Flow Rate Lbs/msec per Injector",null,{"v":1e-05,"d":"1.00E-05"}]
[{"$nulls":9}," ",null," "]
[{"$nulls":16}," "]
[{"$nulls":10}," ",{"$nulls":5}," "]
[{"$nulls":9},"Table for Adjusting Cooling Air density based on temp"]
[{"$nulls":8},"Air Density Adjustment (Actual/Standard Air Density)",null,"Temp F","Density","Ratio","Inverse/ratio"]
[{"$nulls":8},"Standard (59F at 29.92)",null,59,0.002378]
[{"$nulls":10},-15,0.00266,0.893984962406015,1.1185870479394449]
[{"$nulls":10},-10,0.00264,0.9007575757575758,1.1101766190075695]
[{"$nulls":10},-5,0.00262,0.9076335877862596,1.1017661900756939]
[{"$nulls":10},0,0.0026,0.9146153846153846,1.0933557611438183]
[{"$nulls":10},5,0.00258,0.9217054263565891,1.084945332211943]
[{"$nulls":10},10,0.0025599999999999998,0.92890625,1.0765349032800673]
[{"$nulls":10},15,0.0025399999999999997,0.936220472440945,1.0681244743481917]
[{"$nulls":10},20,0.0025199999999999997,0.9436507936507937,1.059714045416316]
[{"$nulls":10},25,0.0025,0.9511999999999999,1.0513036164844407,null,null," "]
[{"$nulls":10},30,0.00248,0.9588709677419355,1.042893187552565]
[{"$nulls":10},35,0.00246,0.9666666666666667,1.0344827586206897]
[{"$nulls":10},40,0.00244,0.9745901639344262,1.0260723296888141]
[{"$nulls":10},45,0.00242,0.9826446280991736,1.0176619007569385]
[{"$nulls":10},50,0.0024,0.9908333333333333,1.0092514718250631]
[{"$nulls":10},55,0.0023799999999999997,0.9991596638655463,1.0008410428931875]
[{"$nulls":10},60,0.002378,1,1]
[{"$nulls":10},65,0.00234,1.0162393162393162,0.9840201850294366]
[{"$nulls":10},70,0.00232,1.025,0.9756097560975611]
[{"$nulls":10},75,0.0023,1.0339130434782609,0.9671993271656855]
[{"$nulls":10},80,0.00228,1.042982456140351,0.9587888982338099]
[{"$nulls":10},85,0.00226,1.052212389380531,0.9503784693019343]
[{"$nulls":10},90,0.00224,1.061607142857143,0.9419680403700588]
[{"$nulls":10},95,0.0022199999999999998,1.0711711711711713,0.9335576114381832]
[{"$nulls":10},100,0.00221,1.0760180995475113,0.9293523969722456]

{"sheet":"Cooling Calculations","index":2,"n_rows":101,"n_cols":19,"rows_kept":101,"merged":[[0,3,1,3],[11,4,12,6],[19,3,20,3],[20,5,21,5],[33,3,34,3],[42,5,43,5]],"flags":["formulas_cached_only"]}
[" ","Choose Air Speed MPH","Climb Duct Speed Coef","True Air Speed MPH",null,"Radiator","Air Density at altitude =",0.07341600000000001,"lb/ft^3","Cp Air","Cp Water","units Cp"]
["Indicated Air Speed =",124,0.35,null,"Ft/Sec","Area in^2","Area ft^2","Air Flow Cubic Feet Sec","Mass Flow Lb/min",0.25,1,"BTU/(Lbm* F)"]
["Engine rpm =",{"v":6000,"d":"6000.00"},"Radiators --->",43.4,{"v":63.653333333333336,"d":"63.65"},{"v":180,"d":"180.00"},1.25,{"v":79.56666666666666,"d":"79.57"},{"v":350.48798400000004,"d":"350.49"}," "]
["Altitude =",{"v":0,"d":"0.00"},"Oil cooler---->",null,{"v":63.653333333333336,"d":"63.65"},{"v":85.5,"d":"85.50"},{"v":0.59375,"d":"0.59"},{"v":37.79416666666667,"d":"37.79"},{"v":166.48179240000002,"d":"166.48"}," ",null," "]
[{"$nulls":6},"Default Values",null,null,"Default Values",null," "]
[null,"Note: Default values for Radiator dimensions",null,"Radiator","Width =",9,9,"Number of Rads =",2,2]
[null,"are for GM evaporator cores",null,null,"Height =",{"v":10,"d":"10.00"},10,"Number of Oil Coolers",1,1]
[null,"Default for Oil cooler is stock RX-7",null," Delta T Rad (F)","Radiator =",70,50]
[{"$nulls":3},"oil Cooler","Width =",{"v":19,"d":"19.00"},19]
[{"$nulls":4},"Height =",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"$nulls":3}," "]
[{"$nulls":3}," Delta T oil  (F)","Oil = ",70,50]
[{"$nulls":4},"Note: if you desire your coolant  flow rate proprational to Engine rpm,. Enter \" =C15\" (without quotation marks) "]
[null,"Pump Factor",185.85," ",{"$nulls":3},"Default Values"]
[null,"Water Pump RPM","Flow gpm",null,"Pump Flow",{"v":38.095238095238095,"d":"38"},"Gallons/Minute ","15-40",null," "]
[null,7080,{"v":38.095238095238095,"d":"38"}," ","Coolant DT ",16,"Degree F","10-15"]
[null," ",null,null,"Cp Coolant",0.8,"Range 0.6 -1.0",0.7,null,"  "]
[]
[{"$nulls":14}," "]
[null,null,"Air Flow","Both Radiators","Q Btu/min","W lb/min","Cp Btu/lbF","Tin_ F  ","Tout_ F"," "," "]
[" ",null,null,"Heat Rejection Capacity",6133.539720000001,{"v":350.48798400000004,"d":"350.49"},0.25,80,150]
[{"$nulls":5},"Needed Heat Rejection",null,null," "]
[{"$nulls":4},"Q Btu/Min",null,"Status","Excess Cooling Capacity"," "]
[{"$nulls":4},6133.539720000001,5982.392728280122,"Cooling",{"v":0.025265307475614618,"d":"2.53%"}]
[" ",{"$nulls":3}," "]
[{"$nulls":4}," ",{"$nulls":9},"HP","Fuel"]
[null,null,"Coolant",null," ",null," ",{"$nulls":7},{"v":195.28537940987135,"d":"195"},{"v":18.165160106113728,"d":"18.17"}]
[null,null," Pump Flow",null,null,"13B Pump"]
[{"$nulls":5},"Flow Rate Gallons/Min","Mass Flow lbm/min"]
[{"$nulls":5},38.095238095238095,317.7142857142857]
[{"$nulls":12},"AF =",12.65,null," ","Temp F =",80," "]
[{"$nulls":12},"Altitude =",0,null," ","Manifold",{"v":29,"d":"29.00"}," "]
[{"$nulls":12},"Gear Ratio ",2.85,null," ","RESULTS"," "," "]
[null," ",null,null,"Q Btu/Min","W lb/Min","Cp Btu/Lb-F (0.6 -1.0)","Tin_F","Tout_F",{"$nulls":4}," ",null," "," ","Radiator Cooler Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"]
[{"$nulls":3},"Heat Rejection Capacity",4066.7428571428572,{"v":317.7142857142857,"d":"317.71"},0.8,210,194,{"$nulls":3},"Engine RPM","Prop RPM",null,"Horse Power/Sec","Gallon/Hour"]
[{"$nulls":4},"Q Btu/Min","Increase Pump Flow?",{"$nulls":6}," "," ",null," "," ","Btu/Min","Btu/Min"]
[{"$nulls":4},4066.7428571428572,"Yes",{"$nulls":6},5500,{"v":1929.8245614035088,"d":"1930"},null,{"v":179.01159779238202,"d":"179"},{"v":16.65139676393758,"d":"16.65"},{"v":5483.860000923442,"d":"5484"},{"v":2741.930000461721,"d":"2742"}]
[{"$nulls":4}," "," ",{"$nulls":6},5600,{"v":1964.9122807017543,"d":"1965"},null,{"v":182.26635411587995,"d":"182"},{"v":16.954149432372812,"d":"16.95"},{"v":5583.566546394781,"d":"5584"},{"v":2791.7832731973904,"d":"2792"}]
[{"$nulls":4}," ",{"$nulls":7},5700,2000,null,{"v":185.52111043937782,"d":"186"},{"v":17.25690210080804,"d":"17.26"},{"v":5683.273091866115,"d":"5683"},{"v":2841.6365459330573,"d":"2842"}]
[{"$nulls":12},5800,{"v":2035.0877192982455,"d":"2035"},null,{"v":188.77586676287567,"d":"189"},{"v":17.559654769243274,"d":"17.56"},{"v":5782.979637337451,"d":"5783"},{"v":2891.4898186687255,"d":"2891"}]
[{"$nulls":12},5900,{"v":2070.175438596491,"d":"2070"},null,{"v":192.03062308637348,"d":"192"},{"v":17.862407437678495,"d":"17.86"},{"v":5882.686182808785,"d":"5883"},{"v":2941.3430914043925,"d":"2941"}]
[null,null,"Air Flow","Oil Cooler","Q Btu/min","W lb/min","Cp Btu/lbF","Tin_ F","Tout_ F",{"$nulls":3},6000,{"v":2105.2631578947367,"d":"2105"},null,{"v":195.28537940987135,"d":"195"},{"v":18.165160106113728,"d":"18.17"},{"v":5982.392728280122,"d":"5982"},{"v":2991.196364140061,"d":"2991"}]
[{"$nulls":4},2913.431367,{"v":166.48179240000002,"d":"166.48"},0.25,80,150,{"$nulls":3},6100,{"v":2140.3508771929824,"d":"2140"},null,{"v":198.54013573336923,"d":"199"},{"v":18.467912774548957,"d":"18.47"},{"v":6082.099273751457,"d":"6082"},{"v":3041.0496368757285,"d":"3041"}]
[{"$nulls":5},"Needed Heat Rejection",null,null," ",{"$nulls":3},6200,{"v":2175.438596491228,"d":"2175"},null,{"v":201.7948920568671,"d":"202"},{"v":18.770665442984185,"d":"18.77"},{"v":6181.805819222792,"d":"6182"},{"v":3090.902909611396,"d":"3091"}]
[null," ",null,null,"Q Btu/Min",null,"Status","Excess Cooling Capacity"," ",{"$nulls":3},6300,{"v":2210.5263157894738,"d":"2211"},null,{"v":205.0496483803649,"d":"205"},{"v":19.073418111419414,"d":"19.07"},{"v":6281.512364694127,"d":"6282"},{"v":3140.7561823470637,"d":"3141"}]
[{"$nulls":4},2913.431367,2991.196364140061,"OverHeat",{"v":-0.025997957898166172,"d":"-2.60%"},{"$nulls":4},6400,{"v":2245.614035087719,"d":"2246"},null,{"v":208.3044047038628,"d":"208"},{"v":19.376170779854647,"d":"19.38"},{"v":6381.218910165462,"d":"6381"},{"v":3190.609455082731,"d":"3191"}]
[{"$nulls":4}," ",{"$nulls":7},6500,{"v":2280.7017543859647,"d":"2281"},null,{"v":211.55916102736066,"d":"212"},{"v":19.67892344828987,"d":"19.68"},{"v":6480.925455636799,"d":"6481"},{"v":3240.4627278183993,"d":"3240"}]
[{"$nulls":12},6600,{"v":2315.7894736842104,"d":"2316"},null,{"v":214.8139173508585,"d":"215"},{"v":19.9816761167251,"d":"19.98"},{"v":6580.632001108133,"d":"6581"},{"v":3290.3160005540667,"d":"3290"}]
[{"$nulls":12},6700,{"v":2350.877192982456,"d":"2351"},null,{"v":218.06867367435632,"d":"218"},{"v":20.28442878516033,"d":"20.28"},{"v":6680.338546579467,"d":"6680"},{"v":3340.1692732897336,"d":"3340"}]
[{"$nulls":12},6800,{"v":2385.964912280702,"d":"2386"},null,{"v":221.3234299978542,"d":"221"},{"v":20.587181453595555,"d":"20.59"},{"v":6780.045092050804,"d":"6780"},{"v":3390.022546025402,"d":"3390"}]
[null,null," ","Over all System Cooling Satus"]
[null,null,"Total BTU of Cooling Capacity",null,9046.971087000002,"Btu/Min","The excessive cooling capacity of the radiators apparently"]
[null,null,"Total BTU of Heat Rejection Needed",null,8973.589092420183,"Btu/Min","enables them to reject some of the heat not rejected by the "]
[{"$nulls":6},"oil cooler"]
[null,null,"Excess Cooling Capacity =",null,{"v":0.008177552351021175,"d":"0.82%"},{"$nulls":6}," "]
[]
[null,null,"Deficient Cooling Capacity =",null,""]
[]
[{"$nulls":11}," "]
{"$rows_empty":40}
["Number radiators"]
[2]
[2]

{"sheet":"Manifold Pressure","index":3,"n_rows":30,"n_cols":14,"rows_kept":30,"hidden":true,"flags":["formulas_cached_only"]}
["AutoTune"]
[null,null,"MAP \"Hg","Map Kpa"]
[null,null,12,40.6283422459893,{"$nulls":6}," "]
[]
[null,null," ",null,null,"=0.039158*(D8*10-31)/((D7+459.7) )"]
[{"$nulls":3},"KPA",null,"air density Manifold","Air Density Altitude"]
[null,null,"Temp  F",80,"\"Hg","lbm/ft^3","lbm/ft^3"]
[null,null,"Map KPA",98.18516042780747,29,0.07135351116038915,0.07341600000000001,null,"=IF(D8<40.6,2,4)"]
[null,null,"Map \"Hg",98.18516042780747,{"v":29,"d":"29.00"}," "," "]
[null,null,"plbm /ft^3",0.0765,null,false,{"$nulls":5},"lbm/time unit"]
[null,null,"Ncylinders",4,{"$nulls":3},"injectors",null,"Duty Cycle ","1 hour","1 sec","1 millsecond"]
[null,null,"CID",160,{"$nulls":3},"#",4,"Limit"]
[null,null,"inj lbm/hr",45,{"$nulls":3},"Rate lbm/hr",44.5489,{"v":1,"d":"100.00%"}]
[null,null,"# inj",1,{"$nulls":3},"Lbm Total 1 hr",178.1956,178.1956,178.1956,0.04949877777777778,{"v":4.9498777777777783e-05,"d":"4.94988E-05"}]
[null,null,"Air/Fuel Ratio",14.7,{"$nulls":5},"Gallons",29.164582651391164,0.008101272958719768,8.101272958719767e-06]
[null,null,"Req Fuel =",8.98885250193867,"millsecond","injector time","for 4 stroke engine"]
[]
[null,null,"Rotor No.",2," ",{"$nulls":8}," "]
[null,null,"E shaft rpm",null,"1 face fires for each 360 deg of e shaft rotation so for 720 deg 2 faces fire or 2 x 40 = 80 cid"]
[null,null,"Displacement/face",40,null,null,"Ve ="]
[null,null,"Faces",3,null,null,{"v":1,"d":"100.00%"},{"$nulls":6}," "]
[{"$nulls":3},"Total Displacement","CF disp","air mass lbm","air mass*Ve","Air/Fuel Ratio","Fuel Mass lbm","injection time"]
[null,null,"Air Volume ",80,0.046296296296296294,0.003303403294462461,{"v":0.003303403294462461,"d":"3.30340E-03"},12,{"v":0.00027528360787187174,"d":"2.75284E-04"},5.561422326582352,"millseconds each for all injectors"]
[{"$nulls":9}," ",null,null," "," "]
[{"$nulls":4},"CFM","lbm/min","lbm/sec",null,"lbm/millsecond",null,"X10",null,null," "]
[null,null,"RPM",2200,101.85185185185185,7.267487247817414,{"v":0.12112478746362357,"d":"1.21125E-01"},14.7,{"v":8.239781460110448e-06,"d":"8.23978E-06"},{"v":0.16646434174804323,"d":"1.66464E-01"},{"v":1.6646434174804323,"d":"1.66464342"}," "]
[{"$nulls":4},"Gal/min"," ",null,null,{"v":0.08091438422367052,"d":"8.09144E-02"},"HP"]
[{"$nulls":4},"gal/hour"," ",null,null,{"v":4.854863053420231,"d":"4.85"},53.93311501163202]
[{"$nulls":8}," "," "," "]
[{"$nulls":8}," "]

{"sheet":"Performance","index":4,"n_rows":3,"n_cols":6,"rows_kept":3,"hidden":true,"flags":["formulas_cached_only"]}
["Propeller","Pitch",null,"Prop Performance based on Pitch"]
[null,72,null,"Engine RPM","Prop RPM","True Air Speed"]
["True Air Speed =",124,null,{"v":6000,"d":"6000.00"},2764.9769585253457,188.52115626309177]