LANCAIR  235/320/360
ANNUAL TYPE CONDITION INSPECTION

Model_________Serial Number _________	Registration Number ________
Tachometer time ________	Total Time ______	Date ________

ENGINE GROUP A	By	Comment	
1.   Check documentation: AD’s.  SB’s.  ARROW, etc.			
2.   Fuel Pressure (boost pump)            psi			
3.   Start-up oil pressure                       psi			
4.   Run engine at 1200 RPM  until oil temperature reaches 140 F			
5.   Idle oil pressure                              psi			
6.   Magneto check DROP  L/H                    R/H                     @1800 RPM			
7.   Suction                                                   Inches of Hg (4-6) normal			
8.   Alternator output                                   Volts                         Amps			
9.   Full power manifold pressure                  Inches @                  RPM			
10.  Check operation of prop governor			
11.  Check all engine guages for proper operation			
12.  Check for general running conditions and vibrations			
13.  Check idle speed and mixture                 rise @                      RPM			
14.  Magneto ground check			
15.  Compression check  #1         /80;  #2         /80;  #3         /80;  #4         /80;			

	By	Comment	
ENGINE GROUP B			
1.   Drain engine oil			
2.   Remove oil filter and screen, check for contaminants			
3.   Check oil breather, inlet and outlet tubes			
4.   Install new oil filter, replace screen gasket.			
5.   Fill crankcase with                       qts,                                         oil			
6.   Clean and gap spark plugs, Rotate plugs top to bottom			
7.   Check  ignition harness for chaffing and general condition			
8.   Check condition of magneto points, replace as necessary			
9.   Check magneto timing in accordance with engine data plate			
10.  Check exhaust system for cracks, security, and condition of gaskets			
11.  Check intake pipes for condition and leaks			
12.  Check condition of air box, clean or replace air filter as necessary			
13.  Check condition of alternate air system and flapper valve			
14.  Check engine baffles and cowling for general condition			
15.  Inspect fuel hoses for general condition			
16.  Inspect oil cooler and hoses for general condition			
17.  Replace or clean fuel filter and screens as necessary			
18.  Check engine vibration isolators for poor condition or deterioration			
19.  Check engine mount for cracks and security to firewall			
20.  Check engine for oil leaks			
21.  Check prop governor for leaks, security, and condition of cable end			
22.  Check starter for security and condition			
23.  Check alternator and mount for security, condition of wiring and belt for       condition and tension			
24.  Check vacuum pump for security and condition			
25.  Check tach cable or wiring for security and condition			
26.  Wash engine as needed.  Do not contaminate vacuum pump or induction system with fluid.			
27.  Lubricate engine controls and check connections and travel			

PROPELLER GROUP C	By	Comment	
1.   Inspect propeller for cracks, nicks, binds, and oil or grease leaks			
2.   Remove minor nicks and dress blades as necessary			
3.   Check mounting bolt torque and safety wiring			
4.   Check blades for looseness in hub			
5.   Inspect spinner, screws, and bulkhead for cracks and condition			
6.   Lubricate propeller per manufacturer’s recommendation			

CABIN GROUP D	By	Comment	
1.   Check seat belts for general condition and defects			
2.   Check battery for electrolyte level and SG and charge			
3.   Check battery vent for security and obstructions			
4.   Clean battery cable terminals if required and reinstall battery			
5.   Check hydraulic power pack and lines for leaks, security, and fluid level			
6.   Check elevator idler arm and bob weight for security and lubricate  rod ends			
7.   Inspect flap motor compartment, rods and motor for proper operation, running current, and lubricate.  Remove attach pin from aft end of flap actuator rod and lubricate.			
8.   Check aileron, elevator push tubes and trim systems and lubricate rod ends			
9.   Check for loose equipment that might foul the controls			
10.  Inspect rudder system, cables, attachments, etc.			
11.  Inspect brake master cylinders and parking brake valve for leakage, free and full extension, and proper operation.  Check fluid level at the master cylinders.			
12.  Check condition of instrument panel wires, hoses, and vacuum filters.			
13.  Check compass for fluid level and correction card			
14.  Check instrument lights			
15.  Check instruments for proper markings, general condition, and security			
16.  Clean inside of cabin and ensure that drain holes are clear			
17.  Inspect fuel lines and tanks for security and leaks			
18.  Inspect pitot static lines			

FUEL SYSTEM GROUP E	By	Comment	
1.   Check fuel transfer pumps for proper operation			
2.   Check fuel tank filters and sump drains for contaminants			
3.   Check all fuel vents for security and obstructions			
4.   Check fuel lines for security, chaffing, and leakage			
5.   Check Fuel tanks and caps for leakage, security, and placards			
6.   Check fuel boost pump for operation, leaks, and security			
7.   Check fuel shutoff valve for operation and leakage			

LANDING GEAR GROUP F	By	Comment	
1.   Place aircraft on jacks			
2.   Clean excess grease off gear legs, struts, and wheels			
3.  Check brake discs and linings for wear or cracks.  Make sure calipers slide freely.			
4.   Check wheels for general condition and cracks			
5.   Check tires for wear, condition, and proper inflation			
6.   Check wheel bearings for corrosion and wear,  re-pack with grease			
7.   Check main gear trailing beams and bolts for wear			
8.   Check main gear weldment for fore and aft end play			
9.   Check compression assemblies and bolts for wear (disassembly required)			
10.  Check nose gear drag link at the knee for wear or hole elongation (disassembly required)			
11.  Check nose gear gas spring for 100# minimum to compress			
12.  Retract the gear checking for wear and freedom of movement of all bearings of gear and drag strut assembly.  Lubricate all moving parts.  Check pressure within limits.			
13.  Check gear doors for fit and security.  Lubricate pivot points and rods.			
14.  Free fall the gear using dump valve.  Check for freedom of movement and overcentering of links.  Check gear using power pack and check pressure down within limits.			
15.  Check nose oleo shimmy damper for proper resistance to movement			
16.  Check nose gear oleo for condition and leakage.  Inflate nose gear oleo to specified pressure unloaded, or strut extension loaded.			
17.  Check nose gear operation when wheel is at slight turning radius and tire or tang do not hang up when gear is retracted			
18.  Check operation of gear position lights and switches			
19.  Check all gear actuators for proper operation and leakage			
20.   Check gear switch is down and dump valve closed.  Remove aircraft from jacks.			

EMPENAGE GROUP G	By	Comment	
1.   Remove exterior inspection covers.  Inspect for security and wear and lubricate torque tubes, cables and bell cranks.  Reinstall inspection covers.			
2.   Inspect rudder hinges and rudder attachment pin safetied			
3.   Inspect trim tabs, elevator hinges, and lubricate			

WING GROUP H	By	Comment	
1.   Remove inspection covers			
2.   Inspect and lubricate all bell cranks, push rods, and  rod ends			
3.   Check all wing attach bolts for security and condition			
4.   Check flaps for general condition and operation			
5.   Check flap actuating rods, bell cranks, hinges, and bearings for condition and lubricate			
6.   Check pitot mast and lines for security and obstruction			
7.   Check ailerons for condition and hinges for wear, lubricate			
8.   Install inspection covers			

ELECTRICAL GROUP I	By	Comment	
1.   Check navigation lights			
2.   Check landing and taxi lights			
3.   Check strobes for proper operation and security			
4.   Check cockpit and instrument lights			
5.   Check pitot heat			
6.   Check ELT for operation:   Battery due date is 			
7.   Transponder check due:			

RADIO GROUP J	By	Comment	
1.   Check radio and electronic equipment for proper installation and secure mounting			
2.   Check wiring and conduits for proper mounting and obvious defects			
3.   Check bonding and shielding for proper installation and condition			
4.   Check antennas for condition, secure mounting, and proper operation			

GENERAL GROUP K	By	Comment	
1.   Check all optional equipment for security and proper operation			
2.   Check all placards			
3.   Check canopy and hardware for general condition and lubricate			
4.   Check composites for signs of delamination, distortion, cracks, damage and lost paint or other evidence of failure			
5.   Clean interior and wash exterior			
6.   All paper work properly signed and Ads and Sbs compliance checked 			
7.  Inspect each installed miscellaneous item that is not otherwise covered by this listing for proper operation and installation.  See FAR Part 43 Appendix D			
8.   Periodically use the dump valve to extend the gear in flight checking for full down and locked condition