{"text_format":"3","workbook":"xls","n_sheets":18,"sheets":["Chart2","Chart4","Sheet1","Sheet2","Sheet3","Sheet4","Sheet5","Sheet6","Sheet7","Sheet8","Sheet9","Sheet10","Sheet11","Sheet12","Sheet13","Sheet14","Sheet15","Sheet16"],"not_rendered":{"charts":2,"external_links":1},"unopened":[{"sheet":"Chart2","index":0,"reason":"not_a_worksheet"},{"sheet":"Chart4","index":1,"reason":"not_a_worksheet"}],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":2,"n_rows":36,"n_cols":16,"rows_kept":36,"flags":["formulas_cached_only"]}
[null,"N654DM",{"$nulls":4},"FLIGHT TEST DATA FORM",{"$nulls":5},"1-888-359-4264"]
[{"$nulls":11},"FAX","1-580-436-6622"]
["DATE","2001-05-26","ENGINE START",null,"TEST START ",null,"MP","RPM","PRESS. ALT",null,"OAT",null,"GEM/JPI","VM1000"]
[null,null,"TIME",1240,"TIME",1315,30.5,2300,8500,null,65,null,"MODEL"]
["Fuel Flow","CHT 1","EGT 1","CHT 2","EGT 2","CHT  3","EGT 3","CHT 4","EGT 4","CHT 5","EGT 5","CHT 6","EGT 6","TIT1","TIT2","IAS (KTS)"]
[22,348,1468,348,1498,328,1478,336,1478,372,1450,336,1432,1260,1294,196]
[21.6,346,1488,342,1508,326,1488,334,1488,368,1460,334,1450,1280,1310,199]
[21.2,346,1505,346,1534,334,1505,334,1505,368,1475,334,1468,1300,1326,199]
[20.6,346,1522,346,1553,334,1522,342,1534,376,1505,342,1494,1310,1336,201]
[20.2,354,1552,346,1570,342,1540,342,1552,382,1512,340,1503,1330,1365,200]
[19.7,354,1570,346,1598,334,1560,340,1570,380,1530,340,1522,1350,1382,198]
[19.4,354,1598,354,1606,334,1588,340,1588,380,1568,340,1552,1400,1402,200]
[19,362,1606,354,1625,338,1598,338,1598,386,1570,338,1560,1410,1410,200]
[18.5,358,1615,346,1625,334,1606,338,1598,386,1578,338,1560,1370,1420,198]
[18.3,358,1615,346,1625,334,1615,338,1598,380,1588,338,1560,1390,1426,198]
[17.8,358,1635,346,1615,334,1606,334,1578,380,1598,334,1548,1380,1426,198]
[17.4,358,1644,338,1606,326,1606,326,1560,380,1598,326,1530,1360,1426,197]
[17.1,346,1622,326,1576,318,1585,318,1536,368,1576,312,1508,1340,1416,194]
[16.7,346,1605,326,1556,318,1566,318,1518,368,1566,312,1502,1320,1398,193]
[16.4,338,1585,326,1548,312,1556,312,1518,358,1556,304,1482,1300,1388,190]
[16,334,1566,312,1518,296,1530,296,1490,354,1530,292,1472,1290,1362,188]
{"$rows_empty":14}
["NAME _____________________","Doug Johnson",null,null,"A/C TYPE __________________","Lancair IV-P",null,null,"ENG. MODEL _______________",null,"Cont TSIO-550B2B",null,"EST. GROSS WT. ___________",null,3200]

{"sheet":"Sheet2","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet4","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet5","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet6","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet7","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet8","index":9,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet9","index":10,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet10","index":11,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet11","index":12,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet12","index":13,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet13","index":14,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet14","index":15,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet15","index":16,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet16","index":17,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}